{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["封面","说明","电气计算汇总表","电气计算","backup"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"封面","index":0,"n_rows":12,"n_cols":4,"rows_kept":12,"merged":[[3,1,3,4],[4,1,4,4],[5,1,5,4]],"flags":["formulas_cached_only"]}
[]
[]
[]
[null,"安 装 工 程"]
[null,"工 程 量 计 算 书"]
[null,"(安装专业)"]
[]
[null,"项目名称:",null,"1号楼6层检验科库房改造"]
[null,"建设单位:"]
[null,"编制单位:"]
[null,"编 制 人:"]
[null,"打印日期:",null,"2019-07-30"]

{"sheet":"说明","index":1,"n_rows":1,"n_cols":36,"rows_kept":1,"merged":[[0,0,1,0],[0,1,1,1]],"flags":["formulas_cached_only"]}
["序号","编  制  说  明  摘  要",{"$nulls":33},"hysd_sm"]

{"sheet":"电气计算汇总表","index":2,"n_rows":19,"n_cols":36,"rows_kept":19,"merged":[[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,0,6],[0,7,1,7],[0,8,1,8],[0,9,1,9],[0,10,1,10],[0,11,1,11]],"flags":["formulas_cached_only"]}
["序号","项目名称","单位","清单量","预算量","项目特征描述",null,"备注","类别","清单编码及属性","清单量","清单计算","hytx_sdjsd436506915277778-1459787",19,{"$nulls":21},"hyaz_sdhzd436506915277778-4693866E-02"]
[{"$nulls":5},"项目名称","工作特征"]
[]
[1,"CT-C-200×150",null,10.58,10.58,"CT-C-200×150",null,null,"CT"]
[2,"二三极五孔插座",null,21,21,"二三极五孔插座",null,null,"插座"]
[3,"600×600LED灯盘 36W",null,11,11,"600×600LED灯盘 36W",null,null,"灯具"]
[4,"接线盒+盖板",null,37,37,"接线盒+盖板",null,null,"盒"]
[5,"单联单控开关",null,2,2,"单联单控开关",null,null,"开关"]
[6,"单联双控开关",null,2,2,"单联双控开关",null,null,"开关"]
[7,"WDZB-BYJ-2.5",null,722.02,749.02,"WDZB-BYJ-2.5",null,null,"配线"]
[8,"WDZB-BYJ-2.5(CT)",null,225.3,274.8,"WDZB-BYJ-2.5(CT)",null,null,"配线"]
[9,"WDZB-BYJ-4",null,26.85,26.85,"WDZB-BYJ-4",null,null,"配线"]
[10,"WDZB-BYJ-4(CT)",null,5.79,10.29,"WDZB-BYJ-4(CT)",null,null,"配线"]
[11,"开关盒",null,25,25,"开关盒",null,null,"配线"]
[12,"AL配电箱",null,1,1,"AL配电箱",null,null,"箱"]
[13,"DN20",null,5.5,5.5,"DN20"]
[14,"SC20(明敷设)",null,182.3,182.3,"SC20(明敷设)"]
[15,"SC20(砖)",null,50.5,50.5,"SC20(砖)"]
[16,"SC25(明敷设)",null,2.98,2.98,"SC25(明敷设)"]

{"sheet":"电气计算","index":3,"n_rows":147,"n_cols":36,"rows_kept":147,"merged":[[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,8,1,8],[0,9,1,9],[0,10,0,11],[0,12,1,12]],"flags":["formulas_cached_only"]}
["系统\n编号","项目名称","配线规格","配线\n根数","配线\n(预算)","预留","配线\n(清单)","小计","单套小计","计   算   式   及   说   明","相同系统",null,"类别",146,null,null,1,{"$nulls":18},"hyaz_sdjsd436506915277778-1459787"]
[{"$nulls":10},"套数","说明"]
[]
["AL配电箱",{"$nulls":12},"$$"]
[null,"AL配电箱",{"$nulls":5},1,1,"1"]
["WL1平面",{"$nulls":12},"$","$"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,43.38,null,43.38,14.46,14.46,"1.82+2.27+3.06+4.01+3.3",{"$nulls":22},"︱HYST-4365070289351857389169‖1.82︱1.82︱C93‖2.27︱2.27︱CA6‖3.06︱3.06︱D00‖4.01︱4.01︱D24‖3.3︱3.3︱D5A"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",4,76.92,null,76.92,19.23,19.23,"6.0+2.94+5.94+2.29+2.06",{"$nulls":22},"︱HYST-4365070289351857389169‖6.0︱6.0︱CB8‖2.94︱2.94︱CCA‖5.94︱5.94︱CDC‖2.29︱2.29︱CEE‖2.06︱2.06︱D48"]
[null,"SC25(明敷设)","WDZB-BYJ-2.5",7,20.86,null,20.86,2.98,2.98,"2.98",{"$nulls":22},"︱HYST-4365070289351857389169‖2.98︱2.98︱D12"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",2,7.44,null,7.44,3.72,3.72,"2.21+1.51",{"$nulls":22},"︱HYST-4365070289351857389169‖2.21︱2.21︱D36‖1.51︱1.51︱D6C"]
["WL1竖直",{"$nulls":12},"$","$"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,15,1.5,10.5,3.5,3.5,"（2.6-1.5）+（2.6-1.4）*2",{"$nulls":22},"︱HYST-4365070289351857389169‖1.82︱1.82︱C93‖2.27︱2.27︱CA6‖3.06︱3.06︱D00‖4.01︱4.01︱D24‖3.3︱3.3︱D5A"]
[null,"SC20(砖)","WDZB-BYJ-2.5",2,4.8,null,4.8,2.4,2.4,"（2.6-1.4）*2",{"$nulls":22},"︱HYST-4365070289351857389169‖2.21︱2.21︱D36‖1.51︱1.51︱D6C"]
[null,"DN20","WDZB-BYJ-2.5",3,16.5,null,16.5,5.5,5.5,"0.5*11",{"$nulls":4},"$"]
[null,"接线盒+盖板",{"$nulls":5},16,16,"11+2+2+1"]
[null,"600×600LED灯盘 36W",{"$nulls":5},11,11,"11",{"$nulls":4},"$"]
[null,"单联单控开关","开关盒",1,2,null,2,2,2,"2",{"$nulls":4},"$"]
[null,"单联双控开关","开关盒",1,2,null,2,2,2,"2",{"$nulls":4},"$"]
["WL2平面",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-4(CT)",3,3.99,null,3.99,1.33,1.33,"1.32+0.01",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(明敷设)","WDZB-BYJ-4",3,19.95,null,19.950000000000003,6.65,6.65,"4.44+2.21",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL2竖直",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-4(CT)",3,6.3,1.5,1.7999999999999998,0.6,0.6,"（2.6-0.5-1.5）",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(砖)","WDZB-BYJ-4",3,6.9,null,6.9,2.3,2.3,"（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},5,5,"5",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,5,null,5,5,5,"5",{"$nulls":4},"$"]
["WL3平面",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,3.99,null,3.99,1.33,1.33,"1.33",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,27.99,null,27.99,9.33,9.33,"9.33",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL3竖直",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,6.3,1.5,1.7999999999999998,0.6,0.6,"（2.6-0.5-1.5）",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,6.9,null,6.9,2.3,2.3,"（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},1,1,"1",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,1,null,1,1,1,"1",{"$nulls":4},"$"]
["WL4平面",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,3.99,null,3.99,1.33,1.33,"4.68",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,27.99,null,27.99,9.33,9.33,"0.3",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL4竖直",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,6.3,1.5,1.7999999999999998,0.6,0.6,"（2.6-0.5-1.5）",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,6.9,null,6.9,2.3,2.3,"（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},1,1,"1",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,1,null,1,1,1,"1",{"$nulls":4},"$"]
["WL5平面",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,17.55,null,17.549999999999997,5.85,5.85,"5.85",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,27.99,null,27.99,9.33,9.33,"0.3",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL5竖直",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,6.3,1.5,1.7999999999999998,0.6,0.6,"（2.6-0.5-1.5）",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,6.9,null,6.9,2.3,2.3,"（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},1,1,"1",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,1,null,1,1,1,"1",{"$nulls":4},"$"]
["WL6平面",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,21.21,null,21.21,7.07,7.07,"7.07",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,27.99,null,27.99,9.33,9.33,"0.3",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL6竖直",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,6.3,1.5,1.7999999999999998,0.6,0.6,"（2.6-0.5-1.5）",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,6.9,null,6.9,2.3,2.3,"（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},1,1,"1",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,1,null,1,1,1,"1",{"$nulls":4},"$"]
["WL7平面",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,24.72,null,24.72,8.24,8.24,"8.24",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,27.99,null,27.99,9.33,9.33,"0.3",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL7竖直",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,6.3,1.5,1.7999999999999998,0.6,0.6,"（2.6-0.5-1.5）",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,6.9,null,6.9,2.3,2.3,"（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},1,1,"1",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,1,null,1,1,1,"1",{"$nulls":4},"$"]
["WL8平面",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,28.2,null,28.200000000000003,9.4,9.4,"9.4",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,27.99,null,27.99,9.33,9.33,"0.3",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL8竖直",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,6.3,1.5,1.7999999999999998,0.6,0.6,"（2.6-0.5-1.5）",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,6.9,null,6.9,2.3,2.3,"（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},1,1,"1",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,1,null,1,1,1,"1",{"$nulls":4},"$"]
["WL9平面",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,14.04,null,14.04,4.68,4.68,"4.68",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,27.99,null,27.99,9.33,9.33,"0.3",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL9竖直",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,6.3,1.5,1.7999999999999998,0.6,0.6,"（2.6-0.5-1.5）",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,6.9,null,6.9,2.3,2.3,"（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},1,1,"1",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,1,null,1,1,1,"1",{"$nulls":4},"$"]
["WL10平面",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,17.58,null,17.580000000000002,5.86,5.86,"5.86",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,27.99,null,27.99,9.33,9.33,"0.3",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL10竖直",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,6.3,1.5,1.7999999999999998,0.6,0.6,"（2.6-0.5-1.5）",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,6.9,null,6.9,2.3,2.3,"（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},1,1,"1",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,1,null,1,1,1,"1",{"$nulls":4},"$"]
["WL11平面",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,21.27,null,21.27,7.09,7.09,"7.09",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,27.99,null,27.99,9.33,9.33,"0.3",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL11竖直",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,6.3,1.5,1.7999999999999998,0.6,0.6,"（2.6-0.5-1.5）",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,6.9,null,6.9,2.3,2.3,"（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},1,1,"1",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,1,null,1,1,1,"1",{"$nulls":4},"$"]
["WL12平面",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,24.75,null,24.75,8.25,8.25,"8.25",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,27.99,null,27.99,9.33,9.33,"0.3",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL12竖直",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,6.3,1.5,1.7999999999999998,0.6,0.6,"（2.6-0.5-1.5）",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,6.9,null,6.9,2.3,2.3,"（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},1,1,"1",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,1,null,1,1,1,"1",{"$nulls":4},"$"]
["WL13平面",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,28.2,null,28.200000000000003,9.4,9.4,"9.4",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,27.99,null,27.99,9.33,9.33,"0.3",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL13竖直",{"$nulls":12},"$","$"]
[null,"线槽配线","WDZB-BYJ-2.5(CT)",3,6.3,1.5,1.7999999999999998,0.6,0.6,"（2.6-0.5-1.5）",{"$nulls":22},"︱HYST-4365070289351857389169‖1.32+0.01︱1.32+0.01︱DC6"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,6.9,null,6.9,2.3,2.3,"（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},1,1,"1",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,1,null,1,1,1,"1",{"$nulls":4},"$"]
["WL14平面",{"$nulls":12},"$","$"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,13.41,null,13.41,4.47,4.47,"4.47",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL14竖直",{"$nulls":12},"$","$"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,14.7,1.5,10.2,3.4,3.4,"（2.6-1.5）+（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},1,1,"1",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,1,null,1,1,1,"1",{"$nulls":4},"$"]
["WL15平面",{"$nulls":12},"$","$"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,17.28,null,17.28,5.76,5.76,"5.76",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL15竖直",{"$nulls":12},"$","$"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,14.7,1.5,10.2,3.4,3.4,"（2.6-1.5）+（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},1,1,"1",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,1,null,1,1,1,"1",{"$nulls":4},"$"]
["WL16平面",{"$nulls":12},"$","$"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,21.42,null,21.42,7.14,7.14,"7.14",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL16竖直",{"$nulls":12},"$","$"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,14.7,1.5,10.2,3.4,3.4,"（2.6-1.5）+（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},1,1,"1",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,1,null,1,1,1,"1",{"$nulls":4},"$"]
["WL17平面",{"$nulls":12},"$","$"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,25.44,null,25.44,8.48,8.48,"8.48",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL17竖直",{"$nulls":12},"$","$"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,14.7,1.5,10.2,3.4,3.4,"（2.6-1.5）+（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},1,1,"1",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,1,null,1,1,1,"1",{"$nulls":4},"$"]
["WL18平面",{"$nulls":12},"$","$"]
[null,"SC20(明敷设)","WDZB-BYJ-2.5",3,29.28,null,29.28,9.76,9.76,"9.76",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
["WL18竖直",{"$nulls":12},"$","$"]
[null,"SC20(砖)","WDZB-BYJ-2.5",3,14.7,1.5,10.2,3.4,3.4,"（2.6-1.5）+（2.6-0.3）",{"$nulls":22},"︱HYST-4365070289351857389169‖4.44︱4.44︱DD8‖2.21︱2.21︱DEA"]
[null,"接线盒+盖板",{"$nulls":5},1,1,"1",{"$nulls":4},"$"]
[null,"二三极五孔插座","开关盒",1,1,null,1,1,1,"1",{"$nulls":4},"$"]
["桥架",{"$nulls":12},"$$"]
[null,"CT-C-200×150",{"$nulls":5},10.58,10.58,"1.33+8.65+(2.6-0.5-1.5)",{"$nulls":22},"︱HYST-4365070289351857389169‖1.33︱1.33︱D89‖8.65︱8.65︱D9C"]
[{"$nulls":14},"$"]

{"sheet":"backup","index":4,"n_rows":3,"n_cols":13,"rows_kept":3,"hidden":true,"flags":["formulas_cached_only"]}
["鸿叶安装图形算量",{"$nulls":5},"$","$","$箱$柜$灯$开关$插座$头$盒$扇$按钮$MR$CT$屏$机$器$泵$端子$模块$接线","$桥架电缆$$$$$$$$$$$$$$$$$","$线槽配线$桥架电缆$选择目标$桥架矿缆$$$$$$$$$$$$$$","$电缆头$接线端子$套管$弯头$三通$异径$管件$开关盒$插座盒$过线盒$$$$$$$$","$0.3[引下]"]
["NEWHYST",{"$nulls":9},20,1]
[{"$nulls":5},"项目代码︱1‖70℃防火阀‖‖‖︱2‖280℃防火阀‖‖‖︱3‖对开多叶调节阀‖‖‖︱4‖风管蝶阀‖‖‖︱5‖风管止回阀‖‖‖︱6‖FK-1双层百叶风口‖‖‖︱7‖FK-2单层百叶风口‖‖‖︱8‖FK-10散流器‖‖‖︱9‖FK-10散流器(配FK-11调节阀)‖‖‖︱10‖管式消声器‖‖‖︱11‖消声静压箱‖‖‖",null,null,"$","$","$","$套管","$"]